Date and time: 2020-11-27, 11:30:15
Size1 = 478 344
CBBBasicAsio::CBBBasicAsio
CBBBasicAsio::MyReStart()
CBBBasicAsio::MyLoadDriver
CBBBasicAsio::MyLoadDriver
Number of Drivers = 5
Driver Name = 'ASIO4ALL v2'
Driver Name = 'Creative Sound Blaster ASIO'
Driver Name = 'ZOOM H and F Series ASIO'
Driver Name = 'ZOOM H and F Series Async ASIO'
Driver Name = 'ZOOM H and F Series Multi ASIO'
Driver 'ASIO4ALL v2' with Index 0 loaded successfully
ASIOInit() = OK
CBBBasicAsio::MyCreateBuffers
Input/Output Channels = 2 2
Buffer Min/Max/Preferred Sizes = 64 2048 64
CBBBasicAsio::CheckSampleRates
Valid Sample Rates: 8000,16000,44100,48000,96000,192000 Hz
Actual Sample Rate = 44100
CBBBasicAsio::CreateBuffers
Input/Output Latency = 3.4 ms, 3.4 ms
Actual Buffer Length = 64
CBBStimulusDefinitionParser::Parse()
CBBBasicAsio::MyStartAsioLoop
ASIOStart() = OK
CBBBasicAsio::MyStopAsioLoop
ASIOStop() = OK
CBBBasicAsio::~CBBBasicAsio
CBBBasicAsio::MyStopAsioLoop
ASIOStop() = OK
CBBBasicAsio::MyDisposeBuffers
ASIODisposeBuffers() = OK
CBBBasicAsio::MyUnloadDriver
ASIOExit() = OK
